JERRY JEFF WALKER BAND BACKLINE RIDER

PLEASE NOTE‑The Equipment listed below is REQUIRED by brand and model
(especially the guitar amplifiers)specific Failure to acquire this specific equipment will be grounds for cancellation of show and forfeiture of deposit, unless approved in advance by Tried & True Music.

If you have any questions or problems, please contact Garrett Guymon at Tried & True Music (512‑477‑0036, fax 512‑477‑0095), 9 a.m. ‑ 5p.m. PLEASE NOTE‑ Jerry Jeff Walker travels with NO road manager or technical personnel.

The Promoter will be responsible for all backline rental costs, including pickup and delivery, unless otherwise specified in your contract

BACKLINE TO INCLUDE.

BASS AMP: ONE bass guitar rig to include:
	ONE solid‑state bass head ‑‑ Gallien‑Krueger 400 RB or 800 RB or SWR 
	ONE bass speaker cabinet‑ Eden, with four 10‑inch speakers.

GUITAR AMPS:
	ONE Trace Elliott (100 Watts), ONE Fender Twin '65 Reissue (Black Face),
	ONE Blues De Ville, and ONE Vox AC 30.

NOTE: If any reason these particular amps cannot be provided, please call
Garrett Guymon at 512‑477‑0036.

DRUMS: One Professional‑quality drum kit (Pearl, Tama, Etc.) To include:
20 or 22 inch kick drum with pedal
10 or 12 inch rack tom (with top and bottom heads in good condition)
14‑inch floor tom (with top and bottom heads in good condition)
5 or 6 1/2 inch snare
14‑inch high hat cymbal (Zildjian cymbals preferred for all)
20‑inch ride cymbal                        "                        “
18 inch thin or medium‑thin crash cymbal                "
16‑inch thin or medium‑thin crash cymbal                "
Drum throne
All necessary hardware and stands
A spare set of heads, in case of emergencies

SOUND AND LIGHT RIDER FOR JERRY JEFF WALKER AND BAND

** PLEASE NOTE -- Jerry Jeff Walker travels with NO road manager or technical personnel.  Please refer any technical questions to Garrett Guymon in our office at (512-477-0036)  **

** PLEASE NOTE – These are our MINIMUM system requirements.  Failure to provide equipment meeting these specifications may result in CANCELLATION of Jerry Jeff Walker’s peformance.  In the event of cancellation, Tried & True Music will retain the contract deposit. **

SOUND:
	HOUSE:		Console at least 18 channel with at least 3 bands EQ (4 preferred)
			1/3 octave EQ on output (2 if PA in stereo)
White, JBL/URIE, or Clark Technic equipment preferred
DIGITAL DELAY:	Delta Lab, SPX 90, Lexicon, etc. equipment preferred – 
Must be full bandwith (No analog)
	SNAKE:		Snake needs split at Monitor Board or stage;  Console MUST be in front  
Engineer will direct placement on site

MAIN SYSTEM:
Main system must feature professional-quality components, i.e. JBL, Gauss, Meyer, etc.
Power amps must feature professional-quality components, i.e. Carver, QSC, Crown
Main system must be active 3-way or 4-way…No passive crossovers except at the tweeter level.
200 to 500 seat venues:			1,500 watt RMS minimum
500 to 1,000 seat venues:		1,500 to 3,000 watts
1,000 to 3,000 seat venues:		10,000 watts

MICS:
VOCALS:  4 Shure SM 58s, or equivalent
INSTRUMENTS:  1 Shure SM 57 (for lead guitar amp), 1 DI with jumper (for bass amp)
DRUMS:	Kick – Sennheiser 421
Snare – Sennheiser 421
Floor Tom – Sennheiser 421
Rack – Sennheiser 421
Hi-Hat – Condenser
Overhead – 2 condensers
MIC STANDS:  6 tall booms, 6 short booms, either Atlas, Beyer, or equivalent

MONITORS:  AT LEAST 6 wedges, bi-amped, PLUS 2 sidefills (stereo)
(SIDEFILLS ARE REQUIRED AT ALL PERFORMANCES), at least 200 watts per box
FOUR MIXES (plus monitor reference); Professional quality 1/3 octave EQ on each mix
(PLEASE NOTE – Jerry Jeff Walker occasionally performs with an extra keyboardist and/or a steel guitarist, each of whom need a separate mix;  Please call Tried & True Music, 512-477-0036 to confirm number of bandmembers before the performance).

LIGHTS:  All lights need to be over 12 feet in height (ceiling permitting)
Configuration:  Side and rear trees… Or side trees and rear truss… Or front and rear truss
200 to 500 seat venues:			24 Par 64	1,000 watt
500 to 1,000 seat venues:		48 Par 64	1,000 watt
1,000 to 3,000 seat venues:		72 Par 64	1,000 watt (or theatrical equiv.)
No follow spots, please
No backwash lighting, please

Three-color wash:  Red White (either Pale Amber or Surprise Pink) and Blue; One spot
Control Console – 12 channel or larger, single scene OK… Smaller equipment quartz lights OK…
No incandescents.

No blackouts between songs, or at show’s end, please.

Jerry Jeff Walker describes his ideal light set-up thus:  “I like the maximum amount of look from the minimum amount of lights.”

PLEASE REFER ANY QUESTIONS OR PROBLEMS TO GARRETT GUYMON AT 
TRIED & TRUE MUSIC (512-477-0036)